// Generated by The stigg true dyno powercurve
RPMTorque=( 0.0, -12.0, 0.0)
RPMTorque=( 1000.0, -30.0, 250.0)
RPMTorque=( 1200.0, -36.0, 255.0)
RPMTorque=( 1400.0, -41.0, 261.0)
RPMTorque=( 1600.0, -46.0, 270.0)
RPMTorque=( 1800.0, -51.0, 280.0)
RPMTorque=( 2000.0, -55.0, 288.8)
RPMTorque=( 2200.0, -59.0, 304.6)
RPMTorque=( 2400.0, -63.0, 334.0)
RPMTorque=( 2600.0, -68.0, 373.9)
RPMTorque=( 2800.0, -75.0, 419.9)
RPMTorque=( 3000.0, -80.0, 472.8)
RPMTorque=( 3200.0, -83.0, 532.7)
RPMTorque=( 3400.0, -90.0, 589.7)
RPMTorque=( 3600.0, -94.0, 658.0)
RPMTorque=( 3800.0, -100.0, 666.3)
RPMTorque=( 4000.0, -105.0, 662.2)
RPMTorque=( 4200.0, -111.0, 658.0)
RPMTorque=( 4400.0, -118.0, 659.4)
RPMTorque=( 4600.0, -125.0, 663.3)
RPMTorque=( 4800.0, -130.0, 654.4)
RPMTorque=( 5000.0, -135.0, 650.6)
RPMTorque=( 5200.0, -140.0, 646.8)
RPMTorque=( 5400.0, -145.0, 638.0)
RPMTorque=( 5600.0, -150.0, 630.4)
RPMTorque=( 5800.0, -157.6, 622.8)
RPMTorque=( 6000.0, -165.0, 616.5)
RPMTorque=( 6200.0, -175.5, 603.8)
RPMTorque=( 6400.0, -183.9, 596.2)
RPMTorque=( 6600.0, -189.1, 581.0)
RPMTorque=( 6800.0, -194.2, 572.2)
RPMTorque=( 7000.0, -198.4, 559.5)
RPMTorque=( 7200.0, -206.7, 551.9)
RPMTorque=( 7400.0, -202.5, 546.8)
RPMTorque=( 7600.0, -205.3, 536.7)
RPMTorque=( 7700.0, -208.1, 530.4)
RPMTorque=( 7800.0, -206.7, 526.6)
RPMTorque=( 7900.0, -205.3, 524.1)
RPMTorque=( 8000.0, -203.9, 522.8)
RPMTorque=( 8100.0, -201.1, 520.3)
RPMTorque=( 8200.0, -192.8, 435.2)
RPMTorque=( 8300.0, -181.6, 354.4)
RPMTorque=( 8400.0, -163.5, 284.8)
RPMTorque=( 8500.0, -139.9, 201.3)
RPMTorque=( 8600.0, -127.3, 116.3)
RPMTorque=( 8700.0, -109.2, 80.0)
RPMTorque=( 8800.0, -92.5, 1.0)
RPMTorque=( 8900.0, -80.0, -100.0)
RPMTorque=( 9000.0, -70.3, -100.0)
RPMTorque=( 9100.0, -64.7, -100.0)
RPMTorque=( 9200.0, -68.9, -100.0)
//
FuelConsumption=3.110e-005   // affected by throttle position and engine speed
FuelEstimate=1.845   // fudge factor for differences between vehicle types (used for lap estimates and AI pit scheduling)
EngineInertia=0.24000   // rotational inertia of engine components
IdleThrottle=.99   // throttle multiplier to help maintain idle speed
IdleRPMLogic=(1000, 1025)   // attempt to maintain idle speed between these RPMs
LaunchEfficiency=0.98   // efficiency (0.0-1.0) of launch control, or 0.0 if N/A
LaunchRPMLogic=(4500, 4900)   // holds RPM in this range before launch (used for AI even if launch control is N/A!)
RevLimitRange=(8600.0, 100.0, 3)
RevLimitSetting=0
RevLimitLogic=2.5                   // RPM range around current setting where rev limiter operates
RevLimitAvailable=1  
40000 or so, and make sure to change [CONTROLS]->UpshiftAlgorithm to fix shifting points)
EngineMapRange=(0, 1, 5)   // 0 = most driveable, max = most power (low gears only) (unimplemented)
EngineMapSetting=1   
EngineBrakingMapRange=(0, 1.250e-04, 6)   // input throttle is ranged from minimum to 100%, with the minimum = setting * step * RPM,
EngineBrakingMapSetting=2   // i.e. if you want 10% throttle at 6000 RPM, set the middle number to 10/6000 = 0.00167
EngineBoostRange=(0.01, 0.01, 12)   
EngineBoostSetting=3   
BoostEffects=(78, 0.14, 0.0015)   // RPM increase per setting, fuel increase (1%) per setting, engine wear rate (101.5%) per setting
BoostTorque=0.00170   // 0.1% less torque per setting (applies to all RPMs)
BoostPower=8.000e-04   // % more horsepower per setting
OptimumOilTemp=98   // degrees Celsius at which engine operates optimally
CombustionHeat=40   // degrees Celsius added per liter of fuel burned
//EngineSpeedHeat=0.00230   // heat added linearly with engine speed
//OilMinimumCooling=0.00950   // heat dissipated without oil/water transfer
EngineSpeedHeat=12.000e-004
OilMinimumCooling=7.90e-003        // heat dissipated without oil/water transfer
OilWaterHeatTransfer=(0.59620, 7.995e-05)   // heat transfer from oil to water (base, w/ engine speed)
//WaterMinimumCooling=1.01298   // base heat dissipated without velocity
WaterMinimumCooling=3.992e-006
RadiatorCooling=(3.892e-04, 3.024e-04)   // cooling rate with velocity (base, per setting)
LifetimeEngineRPM=(8550, 98.0)   // (base engine speed for lifetime, range where lifetime is halved), 180
LifetimeOilTemp=(130.0, 3.0)   // (base oil temp for lifetime, range where lifetime is halved)
LifetimeAvg=32080   // average lifetime in seconds
LifetimeVar=50   // lifetime random variance
EngineEmission=(0, 0.5000, 0.8000)   // where flames and smoke are emitted (relative to ref frame at rear axle)
EngineSound=(0.300, 0.800, -1.2)   // where engine sound is emitted (relative to ref frame at rear axle)
SpeedLimiter=1   // whether there is a pitlane speed limiter
OnboardStarter=1   // whether vehicle restarts when stalled
StarterTiming=(1.50, 0.0, 0.0)   // average and variable cranking time, then blend with starting sound
RamCenter=(0.0, 0.45, -2.9)        // location of ram air intake
RamDraftEffect=2.0                 // multiplier for effect that draft has on ram air velocity
RamEffects=(1.0e-5,1.0e-5,1.0e-5,1.0e-5) // torque % increase per m/s, power % increase per m/s and RPM, fuel increase per m/s, engine wear increase per m/s
