// Pescarolo Courage C60 V10 JUDD 2005
// @JPBS  Juillet 2007 http://team.motorsport.phpnet.org
//-------------------------------------------------------------------
RPMTorque=( 0.0, -14.1, 0.0)
RPMTorque=( 250.0, -20.1, 84.7)
RPMTorque=( 500.0, -26.7, 114.0)
RPMTorque=( 750.0, -33.9, 128.7)
RPMTorque=( 1000.0, -41.5, 143.3)
RPMTorque=( 1250.0, -49.6, 155.3)
RPMTorque=( 1500.0, -58.1, 167.3)
RPMTorque=( 1750.0, -67.0, 184.6)
RPMTorque=( 2000.0, -76.1, 196.6)
RPMTorque=( 2250.0, -85.5, 211.3)
RPMTorque=( 2500.0, -95.0, 231.2)
RPMTorque=( 2750.0, -104.8, 247.2)
RPMTorque=( 3000.0, -114.6, 264.5)
RPMTorque=( 3250.0, -124.5, 284.5)
RPMTorque=( 3500.0, -134.3, 305.8)
RPMTorque=( 3750.0, -144.1, 329.8)
RPMTorque=( 4000.0, -153.8, 358.8)
RPMTorque=( 4250.0, -163.4, 387.0)
RPMTorque=( 4500.0, -172.8, 421.7)
RPMTorque=( 4750.0, -181.9, 447.0)
RPMTorque=( 5000.0, -190.7, 477.6)
RPMTorque=( 5250.0, -199.1, 498.9)
RPMTorque=( 5500.0, -207.2, 520.2)
RPMTorque=( 5750.0, -214.8, 540.2)
RPMTorque=( 6000.0, -221.9, 562.8)
RPMTorque=( 6250.0, -228.5, 580.1)
RPMTorque=( 6500.0, -234.4, 593.5)
RPMTorque=( 6750.0, -239.7, 608.1)
RPMTorque=( 7000.0, -244.4, 613.4)
RPMTorque=( 7250.0, -248.2, 615.0)
RPMTorque=( 7500.0, -251.3, 604.4)
RPMTorque=( 7750.0, -253.5, 588.6)
RPMTorque=( 8000.0, -254.8, 568.0)
RPMTorque=( 8250.0, -255.1, 551.3)
RPMTorque=( 8500.0, -254.5, 536.2)
RPMTorque=( 8750.0, -252.8, 516.8)
RPMTorque=( 9000.0, -250.0, 493.1)
RPMTorque=( 9250.0, -246.0, 464.8)
RPMTorque=( 9500.0, -240.9, 431.7)
RPMTorque=( 9750.0, -234.5, 393.5)
RPMTorque=( 10000.0, -226.8, 350.2)
RPMTorque=( 10250.0, -217.7, 301.4)
RPMTorque=( 10500.0, -207.2, 247.0)
RPMTorque=( 10750.0, -195.3, 186.8)
RPMTorque=( 11000.0, -177.7, 100.7)
FuelConsumption=5.031e-05   // affected by throttle position and engine speed
FuelEstimate=0.70200   // fudge factor for differences between vehicle types (used for lap estimates and AI pit scheduling)
EngineInertia=0.25600   // rotational inertia of engine components
IdleThrottle=0.40000   // throttle multiplier to help maintain idle speed
IdleRPMLogic=(1200, 1450)   // attempt to maintain idle speed between these RPMs
LaunchEfficiency=0   // efficiency (0.0-1.0) of launch control, or 0.0 if N/A
LaunchRPMLogic=(6000, 7000)   // holds RPM in this range before launch (used for AI even if launch control is N/A!)
RevLimitRange=(8000, 100, 16)   
RevLimitSetting=11   
RevLimitLogic=100   // RPM range around current setting where rev limiter operates
RevLimitAvailable=1   // whether to use a rev limit (if 0, you still must have a "rev limit", just make it 40000 or so, and make sure to change [CONTROLS]->UpshiftAlgorithm to fix shifting points)
EngineMapRange=(0, 1, 1)   // 0 = most driveable, max = most power (low gears only) (unimplemented)
EngineMapSetting=1   
EngineBrakingMapRange=(0, 0.0010, 1)   // input throttle is ranged from minimum to 100%, with the minimum = setting * step * RPM,
EngineBrakingMapSetting=0   // the default is 1 * 0.000133 * 15000 RPM = 2% applied throttle at zero input throttle
EngineBoostRange=(0.01000, 1, 10)   
EngineBoostSetting=1   
BoostEffects=(15, 0.0100, 1.0150)   // RPM increase per setting, fuel increase (1%) per setting, engine wear rate (101.5%) per setting
BoostTorque=-0.00410   // 0.4% less torque per setting (applies to all RPMs)
BoostPower=1.600e-04   // % more horsepower per setting
OptimumOilTemp=100   // degrees Celsius at which engine operates optimally
CombustionHeat=40   // degrees Celsius added per liter of fuel burned
EngineSpeedHeat=9.062e-04   // heat added linearly with engine speed
OilMinimumCooling=7.50e-003        // heat dissipated without oil/water transfer
OilWaterHeatTransfer=(3.962e-001,7.925e-005)  // heat transfer from oil to water (base, w/ engine speed)
WaterMinimumCooling=3.962e-003
RadiatorCooling=(1.592e-004, 10.039e-005)
LifetimeEngineRPM=(8640, 180)   // (base engine speed for lifetime, range where lifetime is halved)
LifetimeOilTemp=(105, 2.5000)   // (base oil temp for lifetime, range where lifetime is halved)
LifetimeAvg=15000   // average lifetime in seconds
LifetimeVar=8500   // lifetime random variance
EngineEmission=(0.0000, 0.1000, 0.5000)   // where flames and smoke are emitted (relative to ref frame at rear axle)
EngineSound=(0.20000, 0.6000, -0.5000)   // where engine sound is played (relative to ref frame at rear axle)
SpeedLimiter=1   // whether vehicle has a pitlane speed limiter
OnboardStarter=1   // whether vehicle restarts when stalled
StarterTiming=(1.40, 0.0, 0.0)   // average and variable cranking time, then time to blend with starting sound
