//SCC GTR2
//Judd KV675 3.4L V8
//By Serode
RPMTorque=(    0,  -28.00, -28.00 )
RPMTorque=(  500,  -24.00,  30.00 )
RPMTorque=( 1000,  -22.00,  63.00 )
RPMTorque=( 1500,  -26.00,  96.00 )
RPMTorque=( 2000,  -30.00, 126.00 )
RPMTorque=( 2500,  -36.00, 163.00 )
RPMTorque=( 3000,  -42.00, 199.00 )
RPMTorque=( 3500,  -51.00, 235.00 )
RPMTorque=( 4000,  -60.00, 276.00 )
RPMTorque=( 4500,  -72.00, 319.00 )
RPMTorque=( 5000,  -84.00, 345.00 )
RPMTorque=( 5500,  -98.00, 365.00 )
RPMTorque=( 6000, -111.00, 379.00 )
RPMTorque=( 6500, -127.00, 391.00 )
RPMTorque=( 7000, -142.00, 398.00 )
RPMTorque=( 7500, -157.00, 404.00 )
RPMTorque=( 8000, -173.00, 408.00 )
RPMTorque=( 8500, -190.00, 407.00 )
RPMTorque=( 9000, -208.00, 394.00 )
RPMTorque=( 9500, -225.00, 374.00 )
RPMTorque=(10000, -243.00, 358.00 )
RPMTorque=(10500, -260.00, 337.00 )
RPMTorque=(11000, -280.00, 299.00 )
RPMTorque=(11500, -295.00, 217.00 )
RPMTorque=(12000, -304.00,  44.00 )
RPMTorque=(12500, -320.00, -78.00 )
FuelConsumption=4.426e-005                    // affected by throttle position and engine speed
FuelEstimate=0.849                            // fudge factor for differences between vehicle types (used for lap estimates and AI pit scheduling)
EngineInertia=0.189               
IdleThrottle=1.0                              // throttle multiplier to help maintain idle speed
IdleRPMLogic=( 1300.0, 2000.0 )
LaunchEfficiency=0.978
LaunchRPMLogic=( 7200.0, 9200.0 )
RevLimitRange=( 9800.0, 100.0, 5 )
RevLimitSetting=0
RevLimitLogic=100.0                           // RPM range around current setting where rev limiter operates
EngineMapRange=( 0, 1, 5 )                    // 0 = most driveable, max = most power (low gears only) (unimplemented)
EngineMapSetting=2
EngineBrakingMapRange=(0.0, 0.000125, 6)      // input throttle is ranged from minimum to 100%, with the minimum = setting * step * RPM,
EngineBrakingMapSetting=2                     // the default is 2 * 0.000125 * 16000 RPM = 4% applied throttle at zero input throttle
OptimumOilTemp=104.7                          // degrees Celsius at which engine operates optimally
CombustionHeat=30.0                           // degrees Celsius added per liter of fuel burned
EngineSpeedHeat=1.269e-003                    // heat added linearly with engine speed
OilMinimumCooling=9.212e-004                  // heat dissipated without radiator
OilWaterHeatTransfer=(5.312e-003,1.620e-004)  // heat transfer from oil to water (base, w/ engine speed)
WaterMinimumCooling=3.793e-003                // heat dissipated without radiator
RadiatorCooling=( 2.387e-004, 6.029e-005 )    // cooling rate with velocity (base, per setting)
LifetimeEngineRPM=( 10700.0,339.2 )            // (base engine speed for lifetime, range where lifetime is halved)
LifetimeOilTemp=(122.51,2.88)                 // (base oil temp for lifetime, range where lifetime is halved)
LifetimeAvg=86400                             // average lifetime in seconds
LifetimeVar=43200                             // lifetime random variance
EngineEmission=( 0.0, 0.54, -0.76 )             // where flames and smoke are emitted (relative to ref frame at rear axle)
OnboardStarter=1                              // whether vehicle restarts when stalled
StarterTiming=(1.4, 0.4, 1.5)                 // average and variable cranking time, then time to blend with starting sound
