//SCC F1C
//Mugen MF408S 4L V8 NAE
//v0.5
//RSDG
RPMTorque=(    0,  -30.00, -10.00)
RPMTorque=(  500,  -13.00,  10.00)
RPMTorque=( 1000,  -13.00,  44.00)
RPMTorque=( 1500,  -17.00, 102.00)
RPMTorque=( 2000,  -23.80, 189.00)
RPMTorque=( 2500,  -35.10, 261.00)
RPMTorque=( 3000,  -44.00, 309.00)
RPMTorque=( 3500,  -55.00, 354.00)
RPMTorque=( 4000,  -64.00, 398.00)
RPMTorque=( 4500,  -75.00, 438.00)
RPMTorque=( 5000,  -90.00, 466.00)
RPMTorque=( 5500, -103.00, 487.00)
RPMTorque=( 6000, -117.00, 502.00)
RPMTorque=( 6500, -133.00, 515.00)
RPMTorque=( 7000, -148.00, 525.00)
RPMTorque=( 7500, -165.00, 519.00)
RPMTorque=( 8000, -180.00, 505.00)
RPMTorque=( 8500, -197.00, 489.00)
RPMTorque=( 9000, -212.00, 473.00)
RPMTorque=( 9500, -226.00, 450.00)
RPMTorque=(10000, -240.00, 387.00)
RPMTorque=(10500, -257.00, 248.00)
RPMTorque=(11000, -282.00, -16.00)
FuelConsumption=5.278e-005                    // affected by throttle position and engine speed
FuelEstimate=0.750                            // fudge factor for differences between vehicle types (used for lap estimates and AI pit scheduling)
EngineInertia=0.296
IdleThrottle=1.0                              // throttle multiplier to help maintain idle speed
IdleRPMLogic=(1400.0, 1700.0)
LaunchEfficiency=0.978
LaunchRPMLogic=(6200.0, 7500.0)
RevLimitRange=(9300.0, 100.0, 5)
RevLimitSetting=0
RevLimitLogic=150.0                           // RPM range around current setting where rev limiter operates
EngineMapRange=(0, 1, 5)                      // 0 = most driveable, max = most power (low gears only) (unimplemented)
EngineMapSetting=2
EngineBrakingMapRange=(0.0, 0.000125, 6)      // input throttle is ranged from minimum to 100%, with the minimum = setting * step * RPM,
EngineBrakingMapSetting=2                     // the default is 2 * 0.000125 * 16000 RPM = 4% applied throttle at zero input throttle
OptimumOilTemp=104.7                          // degrees Celsius at which engine operates optimally
CombustionHeat=30.0                           // degrees Celsius added per liter of fuel burned
EngineSpeedHeat=1.647e-003                    // heat added linearly with engine speed
OilMinimumCooling=9.212e-004                  // heat dissipated without radiator
OilWaterHeatTransfer=(5.312e-003,2.103e-004)  // heat transfer from oil to water (base, w/ engine speed)
WaterMinimumCooling=3.793e-003                // heat dissipated without radiator
RadiatorCooling=(2.387e-004, 6.029e-005)      // cooling rate with velocity (base, per setting)
LifetimeEngineRPM=(9500.0,439.2)              // (base engine speed for lifetime, range where lifetime is halved)
LifetimeOilTemp=(122.51,2.88)                 // (base oil temp for lifetime, range where lifetime is halved)
LifetimeAvg=86400                             // average lifetime in seconds
LifetimeVar=43200                             // lifetime random variance
EngineEmission=(0.0, 0.53, 0.0)               // where flames and smoke are emitted (relative to ref frame at rear axle)
OnboardStarter=1                              // whether vehicle restarts when stalled
StarterTiming=(4.5, 0.0, 0.2)                 // average and variable cranking time, then time to blend with starting sound