// Pescarolo Courage C60 V10 JUDD 2005
// @JPBS SEPTEMBRE 2005 V1.02
[GENERAL]
Rules=0
GarageDisplayFlags=7
FeelerFlags=0
Mass=977.1
Inertia=(935.0, 1180.0, 225.0) //(1250.0, 1350.0, 210.0)
FuelTankPos=(0.0, -0.02, -1.180)
FuelTankMotion=(560.0,0.7)
Notes="Pescarolo Courage C60 Hybrid-V10 JUDD 2005"
Symmetric=1
DamageFile=damage
CGHeight=0.095
CGRightRange=(0.500, 0.002, 1)
CGRightSetting=0
CGRearRange=(0.52, 0.000, 5)
CGRearSetting=0
WedgeRange=(0.0, 0.25, 1)
WedgeSetting=0
WedgePushrod=0.0
GraphicalOffset=(0.0, -0.03, 0.0)
Undertray00=(0.95,  -0.00, -1.945)  // offset from center of car, and between axles// LF (Left front corner of splitter) (forward is negative, right is negative)
Undertray01=(-0.95, -0.00, -1.945)  // offset from center of car, and between axles// RF (Right front corner of splitter)
Undertray02=(0.35,  -0.00, 1.855)  // offset from center of car, and between axles // LR (Left rear corner of diffuser)
Undertray03=(-0.35, -0.00, 1.855)  // offset from center of car, and between axles // RR (Right rear corner of diffuser)
Undertray04=(0.35,  -0.00, -2.225)  // offset from center of car, and between axles// Left center front nose
Undertray05=(-0.35, -0.00, -2.225)  // offset from center of car, and between axles// Right center front nose
Undertray06=(0.95,  -0.00, 0.000)  // offset from center of car, and between axles //  Center/bottom of Left rocker panel
Undertray07=(-0.95, -0.00, 0.000)  // offset from center of car, and between axles //  Center/bottom of right rocker panel
Undertray08=(0.35,  -0.00, -1.200)  // offset from center of car, and between axles//  Floor LF corner
Undertray09=(-0.35, -0.00, -1.200)  // offset from center of car, and between axles//  Floor RF corner
Undertray10=(0.35,  -0.00, 0.700)  // offset from center of car, and between axles //  FLoor LR corner
Undertray11=(-0.35, -0.00, 0.700)  // offset from center of car, and between axles //  Floor RR corner
UndertrayParams=(262500.0,11600.0, 4.0) // undertray spring rate, damper rate, and coefficient of friction
TireBrand=LMP900f1c
FrontTireCompoundSetting=1 
RearTireCompoundSetting=1 
FuelRange=(1.0, 1.0, 90)
FuelSetting=50
NumPitstopsRange=(0, 1, 4)
NumPitstopsSetting=3
Pitstop1Range=(1.0, 1.0, 90)
Pitstop1Setting=50
Pitstop2Range=(1.0, 1.0, 90)
Pitstop2Setting=50
Pitstop3Range=(1.0, 1.0, 90)
Pitstop3Setting=50
AIMinPassesPerTick=2
AIRotationThreshold=0.09
AIEvenSuspension=0.0
AISpringRate=0.54
AIDamperSlow=1.2
AIDamperFast=0.4
AIDownforceZArm=0.150
AIDownforceBias=1.0
AITorqueStab=(0.7, 0.9, 0.48)

[FRONTWING]
FWRange=(0.0, 1.0, 10)
FWSetting=6
FWMaxHeight=(0.30)
FWDragParams=(0.0202, 0.0019, 0.0)
FWLiftParams=(-0.3310, -0.0094, 0.00001)
FWLiftHeight=(1.010)
FWLiftSideways=(0.5)
FWLeft=(-0.01, 0.0, 0.0)
FWRight=(0.01, 0.0, 0.0)
FWUp=(0.0, -0.04, -0.001)
FWDown=(0.0, 0.04, 0.001)
FWAft=(0.0, 0.04, -0.04)
FWFore=(0.0, 0.0, 0.0)
FWRot=(0.10, 0.05, 0.15)
FWCenter=(0.00, 0.10, -0.50)

[REARWING]
RWRange=(0.0, 1.0, 20)
RWSetting=13
RWDragParams=(0.0617, 0.00780, 0.0)
RWLiftParams=(-0.3681, -0.01440, 0.00005)
RWLiftSideways=(0.5)
RWLeft=(-0.02, 0.0, 0.0)
RWRight=(0.02, 0.0, 0.0)
RWUp=(0.0, -0.08, -0.002)
RWDown=(0.0, 0.08, 0.002)
RWAft=(0.0, 0.08, -0.08)
RWFore=(0.0, 0.0, 0.0)
RWRot=(0.10, 0.05, 0.15)
RWCenter=(0.00, 0.60, 0.35)

[BODYAERO]
BodyDragBase=(0.305) // 0.305
BodyDragHeightAvg=(0.310)
BodyDragHeightDiff=(0.535)
BodyMaxHeight=(0.20)
BodyLeft=(-0.7, 0.0, 0.0)
BodyRight=(0.7, 0.0, 0.0)
BodyUp=(0.0, -1.5, 0.0)
BodyDown=(0.0, 1.5, 0.0)
BodyAft=(0.0, 0.10, -1.00)
BodyFore=(0.000, -0.383, 0.455)
BodyRot=(2.0, 1.5, 1.0)
BodyCenter=(0.0, 0.251, -2.071)//-1.871
RadiatorRange=(0.0, 1.0, 5)
RadiatorSetting=3
RadiatorDrag=(0.004)
RadiatorLift=(0.011)
BrakeDuctRange=(0.0, 1.0, 7)
BrakeDuctSetting=4
BrakeDuctDrag=(0.006)
BrakeDuctLift=(0.014)

[DIFFUSER]
DiffuserBase=(-0.625, -7.000, 90.000) //   0.450 / 50
DiffuserFrontHeight=(0.202)
DiffuserRake=(0.000, -10.0, 300.0)
DiffuserLimits=(0.010, 0.100, 0.065)
DiffuserStall=(0.0, 1.0)  
DiffuserSideways=(0.5)
DiffuserCenter=(0.0, 0.01, -1.096)  // -1.096

[SUSPENSION]
PhysicalModelFile=C60.SP
ApplySlowToFastDampers=0
AdjustSuspRates=1
AlignWheels=1
FrontWheelTrack=0.0
RearWheelTrack=0.0
LeftWheelBase=0.0
RightWheelBase=0.0
SpringBasedAntiSway=1
FrontAntiSwayBase=0.0
FrontAntiSwayRange=(0.0, 5000.0, 51)
FrontAntiSwaySetting=24
FrontAntiSwayRate=(0.0, 0.0)
RearAntiSwayBase=0.0
RearAntiSwayRange=(0.0, 5000.0, 41)
RearAntiSwaySetting=8
RearAntiSwayRate=(0.0, 0.0)
FrontToeInRange=(-2.0, 0.1, 41)
FrontToeInSetting=18
RearToeInRange=(-2.0, 0.1, 41)
RearToeInSetting=22
LeftCasterRange=(-2.0, 0.1, 81)
LeftCasterSetting=58
RightCasterRange=(-2.0, 0.1, 81)
RightCasterSetting=58
LeftTrackBarRange=(0.0, 0.0, 0)
LeftTrackBarSetting=0
RightTrackBarRange=(0.0, 0.0, 0)
RightTrackBarSetting=0

[CONTROLS]
SteerLockRange=(5.0, 0.5, 35)
SteerLockSetting=16
RearBrakeRange=(0.200, 0.005, 121)
RearBrakeSetting=39
BrakePressureRange=(0.50, 0.01, 51)
BrakePressureSetting=50
HandbrakePressRange=(0.00, 0.05, 1)
HandbrakePressSetting=0
AutoUpshiftGripThresh=0.63
AutoDownshiftGripThresh=0.63
TractionControlGrip=(1.00, 0.20)
TractionControlLevel=(0.30, 0.90)
ABS4Wheel=1
ABSGrip=(1.00, 0.20)
ABSLevel=(0.30, 0.90)

[ENGINE]
Normal=C60.eng
RestrictorPlate=C60

[DRIVELINE]
ClutchInertia=0.0287
ClutchTorque=1200.0
ClutchWear=0.0
ClutchFriction=13.708
BaulkTorque=777.1
AllowManualOverride=1
SemiAutomatic=1
UpshiftDelay=0.029
UpshiftClutchTime=0.19
DownshiftDelay=0.029
DownshiftClutchTime=0.19
WheelDrive=REAR
GearFile=C60.GRB
FinalDriveSetting=1
ReverseSetting=0
ForwardGears=6
Gear1Setting=5
Gear2Setting=10
Gear3Setting=15
Gear4Setting=19
Gear5Setting=22
Gear6Setting=26
DiffPumpTorque=200.0
DiffPumpRange=(0.00, 0.05, 21)
DiffPumpSetting=9
DiffPowerRange=(0.00, 0.05, 21)
DiffPowerSetting=6
DiffCoastRange=(0.00, 0.05, 21)
DiffCoastSetting=9
DiffPreloadRange=(80.0, 20.0, 5)
DiffPreloadSetting=2

[FRONTLEFT]
BumpTravel=-0.008
ReboundTravel=-0.111
BumpStopSpring=290815.4
BumpStopRisingSpring=6.50e6
BumpStopDamper=3763.5
BumpStopRisingDamper=7.00e5
BumpStage2=0.125
ReboundStage2=-0.125
FrictionTorque=1.50
SpinInertia=1.144
CGOffsetX=0.000
PushrodSpindle=(-0.050, -0.100, 0.000)
PushrodBody=(-0.580, 0.170, 0.0)
CamberRange=(-6.0, 0.1, 81)
CamberSetting=28
PressureRange=(90.0, 1.0, 106)
PressureSetting=45
PackerRange=(0.000, 0.001, 41)
PackerSetting=0
SpringRange=(50000.0, 5000.0, 31)
SpringSetting=19
RideHeightRange=( 0.05, 0.001, 41 )
RideHeightSetting=0
SlowBumpRange=(1000.0, 100.0, 16)
SlowBumpSetting=7
FastBumpRange=(700.0, 100.0, 11)
FastBumpSetting=7
SlowReboundRange=(1600.0, 200.0, 16)
SlowReboundSetting=11
FastReboundRange=(1200.0, 200.0, 11)
FastReboundSetting=8
BrakeDiscRange=(0.037, 0.000, 0)
BrakeDiscSetting=0
BrakePadRange=(0, 1, 5)
BrakePadSetting=2
BrakeDiscInertia=1.223
BrakeOptimumTemp=750.0           
BrakeFadeRange=750.0             
BrakeWearRate=4.822e-011         
BrakeFailure=(1.43e-002,5.40e-004)  
BrakeTorque=4015.0          
BrakeHeating=6.012e-004        
BrakeCooling=(1.745e-002,2.334e-004)
BrakeDuctCooling=0.633e-004       

[FRONTRIGHT]
BumpTravel=-0.008
ReboundTravel=-0.111
BumpStopSpring=290815.4
BumpStopRisingSpring=6.50e6
BumpStopDamper=3763.5
BumpStopRisingDamper=7.00e5
BumpStage2=0.125
ReboundStage2=-0.125
FrictionTorque=1.50
SpinInertia=1.144
CGOffsetX=0.000
//PushrodSpindle=(0.050, -0.150, 0.000)
//PushrodBody=(-0.080, 0.170, 0.0)
PushrodSpindle=(0.050, -0.100, 0.000)
PushrodBody=(0.580, 0.170, 0.0)
CamberRange=(-6.0, 0.1, 81)
CamberSetting=28
PressureRange=(90.0, 1.0, 106)
PressureSetting=45
PackerRange=(0.000, 0.001, 41)
PackerSetting=0
SpringRange=(50000.0, 5000.0, 31)
SpringSetting=19
RideHeightRange=( 0.05, 0.001, 41 )
RideHeightSetting=0
SlowBumpRange=(1000.0, 100.0, 16)
SlowBumpSetting=7
FastBumpRange=(700.0, 100.0, 11)
FastBumpSetting=7
SlowReboundRange=(1600.0, 200.0, 16)
SlowReboundSetting=11
FastReboundRange=(1200.0, 200.0, 11)
FastReboundSetting=8
BrakeDiscRange=(0.037, 0.000, 0)
BrakeDiscSetting=0
BrakePadRange=(0, 1, 5)
BrakePadSetting=2
BrakeDiscInertia=1.223
BrakeOptimumTemp=750.0           
BrakeFadeRange=750.0             
BrakeWearRate=4.822e-011         
BrakeFailure=(1.43e-002,5.40e-004)  
BrakeTorque=4015.0          
BrakeHeating=6.012e-004        
BrakeCooling=(1.745e-002,2.334e-004)
BrakeDuctCooling=0.633e-004       

[REARLEFT]
BumpTravel=-0.017
ReboundTravel=-0.153
BumpStopSpring=290815.4
BumpStopRisingSpring=6.50e6
BumpStopDamper=3763.5
BumpStopRisingDamper=7.00e5
BumpStage2=0.125
ReboundStage2=-0.125
FrictionTorque=1.50
SpinInertia=1.226
CGOffsetX=-0.030
PushrodSpindle=(-0.050, -0.125, 0.000)
PushrodBody=(-0.560, 0.170, 0.0)
CamberRange=(-6.0, 0.1, 81)
CamberSetting=40
PressureRange=(90.0, 1.0, 106)
PressureSetting=40
PackerRange=(0.000, 0.001, 61)
PackerSetting=0
SpringRange=(50000.0, 5000.0, 31)
SpringSetting=19
RideHeightRange=( 0.06, 0.001, 41 )
RideHeightSetting=20
SlowBumpRange=(1000.0, 100.0, 16)
SlowBumpSetting=9
FastBumpRange=(700.0, 100.0, 11)
FastBumpSetting=6
SlowReboundRange=(1600.0, 200.0, 16)
SlowReboundSetting=12
FastReboundRange=(1200.0, 200.0, 11)
FastReboundSetting=9
BrakeDiscRange=(0.037, 0.000, 0)
BrakeDiscSetting=0
BrakePadRange=(0, 1, 5)
BrakePadSetting=2
BrakeDiscInertia=1.223
BrakeOptimumTemp=750.0            
BrakeFadeRange=750.0               
BrakeWearRate=4.822e-011        
BrakeFailure=(1.43e-002,5.40e-004)  
BrakeTorque=3905.0         
BrakeHeating=6.012e-004           
BrakeCooling=(1.745e-002,2.334e-004)
BrakeDuctCooling=0.633e-004  

[REARRIGHT]
BumpTravel=-0.017
ReboundTravel=-0.153
BumpStopSpring=290815.4
BumpStopRisingSpring=6.50e6
BumpStopDamper=3763.5
BumpStopRisingDamper=7.00e5
BumpStage2=0.125
ReboundStage2=-0.125
FrictionTorque=1.50
SpinInertia=1.226
CGOffsetX=0.030
PushrodSpindle=(0.050, -0.125, 0.000)
PushrodBody=(0.560, 0.170, 0.0)
CamberRange=(-6.0, 0.1, 81)
CamberSetting=40
PressureRange=(90.0, 1.0, 106)
PressureSetting=40
PackerRange=(0.000, 0.001, 61)
PackerSetting=0
SpringRange=(50000.0, 5000.0, 31)
SpringSetting=19
RideHeightRange=( 0.06, 0.001, 41 )
RideHeightSetting=20
SlowBumpRange=(1000.0, 100.0, 16)
SlowBumpSetting=9
FastBumpRange=(700.0, 100.0, 11)
FastBumpSetting=6
SlowReboundRange=(1600.0, 200.0, 16)
SlowReboundSetting=12
FastReboundRange=(1200.0, 200.0, 11)
FastReboundSetting=9
BrakeDiscRange=(0.037, 0.000, 0)
BrakeDiscSetting=0
BrakePadRange=(0, 1, 5)
BrakePadSetting=2
BrakeDiscInertia=1.223
BrakeOptimumTemp=750.0            
BrakeFadeRange=750.0               
BrakeWearRate=4.822e-011        
BrakeFailure=(1.43e-002,5.40e-004)  
BrakeTorque=3905.0         
BrakeHeating=6.012e-004           
BrakeCooling=(1.745e-002,2.334e-004)
BrakeDuctCooling=0.633e-004  


